{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Certificate_Template"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":772,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Certificate_Template","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[[0,0,2,8],[38,0,38,8],[39,0,39,8],[5,0,5,1],[5,2,5,3],[5,5,5,6],[5,7,5,8],[6,0,6,1],[6,2,6,3],[6,5,6,6],[6,7,6,8],[7,0,7,1],[7,2,7,3],[7,5,7,6],[7,7,7,8],[8,0,8,1],[8,2,8,3],[8,5,8,6],[8,7,8,8],[9,0,9,1],[9,2,9,3],[9,5,9,6],[9,7,9,8],[10,0,10,1],[10,2,10,3],[10,5,10,6],[10,7,10,8],[11,0,11,1],[11,2,11,3],[11,5,11,6],[11,7,11,8],[12,0,12,1],[12,2,12,3],[12,5,12,6],[12,7,12,8],[13,0,13,1],[13,2,13,3],[13,5,13,6],[13,7,13,8],[14,0,14,1],[14,2,14,3],[14,5,14,6],[14,7,14,8],[15,0,15,1],[15,2,15,3],[15,5,15,6],[15,7,15,8],[16,0,16,1],[16,2,16,3],[16,5,16,6],[16,7,16,8],[17,0,17,1],[17,2,17,3],[17,5,17,6],[17,7,17,8],[18,0,18,1],[18,2,18,3],[18,5,18,6],[18,7,18,8],[19,0,19,1],[19,2,19,3],[19,5,19,6],[19,7,19,8],[20,0,20,1],[20,2,20,3],[20,5,20,6],[20,7,20,8],[24,7,24,8],[21,0,21,1],[21,2,21,3],[21,5,21,6],[21,7,21,8],[22,0,22,1],[22,2,22,3],[22,5,22,6],[22,7,22,8],[27,0,27,1],[3,0,3,3],[3,5,3,8],[4,0,4,1],[4,2,4,3],[4,5,4,6],[4,7,4,8],[23,0,23,1],[23,2,23,3],[23,5,23,6],[23,7,23,8],[24,0,24,1],[24,2,24,3],[24,5,24,6]]}
[]
[]
[]
["DEVICE UNDER TEST",null,null,null,null,"CALIBRATION"]
["Device Identifier",null,"BIG OIL TANK",null,null,"Date of Calibration",null,"27-JUL-2022"]
["Serial Number",null,"0459",null,null,"Operator"]
["Manufacturer",null,null,null,null,"Location"]
["Model",null,null,null,null,"Ambient Temperature",null,"20.00 °C"]
["Sensor Type",null,"Gauge",null,null,"Ambient Pressure",null,"1008.00 mbar"]
[null,null,null,null,null,"Ambient Humidity",null,"70.00%"]
[]
[]
["TEST EQUIPMENT",null,null,null,null,"ADDITIONAL SENSORS",null,"1"]
["MAIN CALIBRATOR",null,null,null,null,"Manufacturer",null,"Druck"]
["Manufacturer",null,"Druck",null,null,"Model",null,"DPI610E-PC-14G"]
["Model",null,"DPI610E-PC-14G",null,null,"Serial Number",null,"0012222"]
["Serial Number",null,"0012121908",null,null,"Date of Calibration",null,"15-MAR-2022"]
["Date of Calibration",null,"15-MAR-2022",null,null,"Sensor Type",null,"Gauge"]
["Calibration Interval",null,"365 days",null,null,"RANGE",null,"-1.14 to 39.77 User"]
[]
[]
["RANGE",null,null,null,null,"TOLERANCE"]
["Input",null,"0.000 bar = 0.000 MSf@20 8.800 bar = 10.000 MSf@20",null,null,"Test Point",null,"5.00 %Span"]
["Output",null,"4.000 mA = 0.000 FtS@20 20.000 mA = 37.270 FtS@20",null,null,"Pass/Fail",null,"0.10 %Span"]
["Relationship",null,"Linear",null,null,"Adjustment",null,"0.07 % Span"]
[]
[]
["AS FOUND",null,null,null,null,null,"Result:","PASS"]
[null,null,"Expected Input","Actual Input","Expected Output","Actual Output","Error","Status"]
[null,null,"CH1","CH1","CH2","CH2"]
[null,null,"MSf@20","MSf@20","FtS@20","FtS@20","FtS@20"]
[null,"1","0.00000","0.00016","0.00061","-0.01144","-0.03234","PASS"]
[null,"2","2.50000","2.51195","9.36204","9.34103","-0.05639","PASS"]
[null,"3","5.00000","5.02168","18.71579","18.69728","-0.04965","PASS"]
[null,"4","7.50000","7.47053","27.84266","27.84952","0.01840","PASS"]
[null,"5","10.00000","9.99997","37.26987","37.25549","-0.03859","PASS"]
[]
[]
["CALIBRATION REMARKS"]
["OK"]
[]
[]
["Approved:"]
["Date:"]